# Introduction

The project is to create an accurate, low distortion signal generator for sine, square and triangle waveforms, alongside a frequency meter for the same. This will be implemented using an ARM processor carrier board from ST Microelectronics (STM32F407VGT6) fitted with various peripherals.

The project will be split into two parts, software and hardware. From the combination of these two parts, the maximum possible frequency range for the waveforms needs to be achieved, and again for the frequency meter using the lowest power achievable. The input signal to the frequency meter on the board is provided by the hardware and displays the frequency on the LCD display. Further work on the product may include using the LCD screen, I2C connector, USB connector, and Direct Digital Synthesis (DDS) using a AD9850 chip to generate accurate pulse and arbitrary functions.

Environment consideration…

Input protection, output impedance, power supplies

Power consumption – minimisation of power

Component list, housing, form factor

# Specification

## Level 2 Requirements

* Generate a sine wave from 0.01Hz to ?HZ with a maximum amplitude of +/- 12V.
* Generate a square wave from 0.01Hz to ?Hz with a maximum amplitude of +/- 12V.
* Generate a triangle wave from 0.01Hz to ?Hz with a maximum amplitude of +/- 12V.
* Measure the frequency of sine, square and triangle waves from 0.01Hz to ?Hz with a minimum signal of 0.1V rms.
* Control the amplitude of sine, square and triangle waves by sending control signals to a digital potentiometer, which will control the gain of the amplifier circuit.
* Create a pulse generator from ?Hz to ?Hz with a maximum amplitude of +12V.
* Measure the duty cycle for digital waveforms.
* Vary the duty cycle for digital waveforms.
* Amplitude modulate an input signal by using a sine wave to send control signals to a digital potentiometer, which will control the gain of the amplifier circuit.
* Frequency modulate an input signal by feeding it into the ADC and using the resulting values to vary the frequency of the output signal, based on a sine wave with a fixed frequency.

## Further Requirements

* Generate square waves using DDS on the AD9850 chip.
* Generate sine waves using DDS on the AD9850 chip.
* Create a random noise generator using the internal PR sequence generator.

# Software Design/Implementation

## Tasks so Far

After following a few brief example programs provided as part of lab script 1 [REF ME], we started the wave generation section.

To start with we generated a square wave with a 50:50 duty cycle, by outputting a high for 5 milliseconds followed by a low for 5 milliseconds on GPIO pin PA0. This gave a nice clean square wave which we viewed on the oscilloscope, and measured the frequency and period. The theoretical period was 10 milliseconds giving a 100Hz frequency, however when measured on the oscilloscope the period was 32 milliseconds and the frequency at 31.25Hz. Consequently this method of setting the frequency is very poor in terms of accuracy, and therefore unsuitable given our specification.

## Tasks Still to Complete

# Hardware Design/Implementation

## Tasks so Far

The hardware team so far has been working together to investigate a variety of circuits for generation of the square, triangle and sine waves. Their main focus has been trying to generate a 1MHz signal from each circuit, with 100kHz being the absolute minimum requirement to achieve the level one design. They have managed to generate all three types of signal with varying degrees of success in terms of the highest frequency obtained.

**Square-waves**

Three circuits have been utilised for square wave generation so far: a Schmitt trigger configuration and two astable multivibrator circuits as described on the Intersil datasheet . Figure 1 shows the Schmitt trigger circuit, with a LM318 op-amp; a TL071 was also used though it has a lower slew rate than the LM318 meaning it would be less likely to achieve the 1MHz goal. Figure 2, below, shows the output from this circuit set up as given in the lab script to give a 400Hz frequency output.




Figure 2 Oscilloscope display for the Schmitt trigger

As can been seen this configuration gives a very clear square wave output. The next task was to work out whether to change the capacitor or the resistor to vary the frequency as both components effect this. Figures 3 and 4 show the generation of a 100Hz wave, with figure 3 having changed the capacitor and figure 4 using a different resistor to that in the initial circuit. It is quite clear that at low frequencies it doesn’t matter which component is changed as both give the same result.





Figure Output due to changing the capacitor Figure Output due to changing the resistor

It was then decided to try a frequency of 10kHz again varying just one of the components. Again both produced the same results however, as can be seen in Figures 5 and 6, the slew rate of the op-amp became a limiting factor and thus the rise and fall times for the square wave have increased significantly. This circuit is clearly unsuitable for use in the function generator as it is unable to produce precise squarewaves at even moderately high frequencies.





Figure 5 Output with fixed resistor value Figure 6 Output with a fixed capacitor value

The next circuit investigated utilised the 7555 timer IC as part of a multivibrator circuit, set up following figure 2B from the datasheet. This configuration allows for the duty cycle to be varied as well as the frequency, however it was quickly found that trying to adjust one would also cause the other to change and that it would be difficult to achieve a fixed 50/50 duty cycle while also being able to change the frequency. Fortunately the datasheet provided another circuit (Figure 2A from ) that had a fixed 50/50 duty cycle, this circuit has two outputs, both of which have been considered. Figure 7 shows both of these outputs for a 1kHz squarewave, each one giving a very clean signal.




Figure 7 Output from the 7555 circuit set up to give a fixed 50/50 duty cycle

The next step was to attempt to output a 100kHz signal, this is show in figure 8.




Figure 8 The 7555 circuit outputting an approximate 100kHz wave

Here the outputs have become much noisier and the alternate output’s rise time is affected drastically by the capacitor. Ultimately a 700kHz output was obtained, though the signal at this point had a noticeable rise time and was fairly noisy, the other output at this frequency was giving a sawtooth wave, figure 9 shows the scope display.




Figure 9 The maximum possible value from the 7555 circuit

The team found that a frequency much higher than this would be hard to obtain as both the resistor (100Ω) and the capacitor (100pF) were heading towards being dominated by the internal resistance and capacitance of the wiring used to create the circuit. It was also decided to check that this circuit operated correctly at very low frequencies. Figure 10 shows a 0.01Hz signal. The scope was unable to measure such low frequencies however a very clean signal was obtained meaning that this circuit could be used if the software team stuggled to generate lower frequency signals.




Figure 10 Using the 7555 to generate a very low frequency signal

After some research on the internet the team came across a circuit designed to generate a triangle wave . Changing R1 to a variable potentiometer allowed the frequency to be adjusted. Currently the team have achieved a top frequency of about 500Hz, they have been limited by the fact that as the frequency increases the amplitude of the output waveform decreases. Beyond 500Hz the amplitude was so small that the signal barely registered on the oscilloscope.

* Triangle wave from 7555 (including square wave)
  + 500Hz – amplitude decreases with increasing frequency
* Sine wave from Wien Bridge oscillator
  + Changed capacitor for each 10x frequency change

## Tasks Still to Complete

**Switching circuit**

Switching circuits are supposed to be used for designing an integrated circuit for changing between three kinds of waveforms and vary their frequencies. Multiple switch or analogue switches controlled by processer such as DG201 quad SPST Switch and DG409 dual 4--‐1 mul0plexer will be used. This task will base on the final specific design of the oscillator circuits and the relationship between frequency of waveforms and components in oscillator circuit. For example, change the value capacitors is one of the solutions of changing sine wave frequency for Wien Bridge oscillator. In this case, circuit like figure [1] might be used and resistors connected with Half DG409 will be replaced by different value capacitors.

Limitation of this solution is that frequencies could not be varied into specific values, only several fixed value are available. In order to solve this, team will try to figure out the way of using other designs like variable resistors or using digital potentiometer.

**Compare CMOS squarewave oscillator with 7555**

4093 CMOS is another square wave generator which was suggested to use in lab script. Although team already got a working 7555 square wave oscillator, some limitations of that circuit still exist. It is worth to build a CMOS oscillator and see what will happen and compare with 7555 oscillator.

**Better triangle wave generator**

Current triangle wave generator is just able to generate a fixed-frequency triangle wave. Team haven’t found the relationship between its frequency and components in the circuit.

Team planning to try to build a Schmitt trigger circuit and add an inverter at the output of trigger circuit for generating triangle wave. Circuit diagram figure [2] is added in appendix.

**Pulse generator**

This is a level 2 requirement. Team planning to use 7555 timer to build a pulse generator, circuit diagram figure [3] is added in appendix.

**Investigate other sine wave generators**

Wien bridge oscillator is the only circuit team have tried for sine wave generator. It works but has limitations when team tried to get high frequency waveform. In order to get higher frequency sine wave, it is necessary to try other kinds of sine wave oscillators such as RC Phase Shift Oscillator and Digital Shift register based Sine Wave Oscillator.

**Create amplifier and dc offset stage**

In order to control waveforms’ amplitude, team planning to design an amplifier circuits with variable resistors to change gain of the circuit. Circuit diagram figure [4] is added in appendix.

**Comparator with and without hysteresis**

Comparator would be used for convert waves produced by oscillators into digital signals. Team plan to build a circuit as figure [5] shows. Output signal of LM 319 will be connected into an N bit counter. Counter will count for N seconds and give output signals to GPIO. Hardware team will build both comparator circuits that with and without hysteresis and compare difference between them and decide which one should be used as final design.

**Detail of design**

* Environment consideration
* Input protection, output impedance, power supplies
* Power consumption – minimisation of power
* Component list, housing, form factor

# Gannt Chart

# Appendix




Figure 1 Schmitt trigger oscillator circuit diagram




Figure. 11 <http://www.elec.york.ac.uk/internal_web/meng/yr3/modules/Design_Construction/Generating%20Signals.pdf>




Figure. 12 <http://www.circuitstoday.com/wp-content/uploads/2009/09/triangular-waveform-using-schmitt-trigger-and-integrator.jpg>





Figure. 13 <http://www.talkingelectronics.com/projects/555/Page2-555.html> 

Figure. 14 <http://homepages.which.net/~paul.hills/Circuits/PowerServo/PowerServo.html>




Figure .15 <http://www.elec.york.ac.uk/internal_web/meng/yr3/modules/Design_Construction/Measuring%20Frequency.pdf>